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Feritoia con portello a filo ricavato dal taglio
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Feritoia, su pali min d.76 – max d.450, dimensioni apertura da 200x60 a 600x150, attacco m.a.t. e 2 traversini per fissaggio morsettiera interno palo, portello in acciaio con serratura vite triangolare.
N.B. verificare idoneità strutturale palo

Versione IP30 “protezione contro l’introduzione di corpi solidi”

Versione IP44 “protezione contro l’introduzione di corpi solidi e la penetrazione di acqua”

Versione rinforzata con 2 piatti interni laterali saldati, per ripristinare la capacità strutturale della sezione integra

Opening with flush door made from cutting 
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Opening on columns minimum d.76 – max d.450, opening dimensions form 200x60 to 600x150, earth connection and 2 supports for unction box fixing inside the column, steel door with triangular screw locking device.

N.B. verify structural suitability of the column

 IP30 version “protection against introduction of solid pieces”

IP44 version “protection against introduction of solid pieces and water penetration”

Reinforced version with 2 side flat irons welded inside, to restore the structural capacity of the whole section 
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